|  |  |
| --- | --- |
| Model | TC-28SA |
| Cutting capacity(mm) | 90°W:360 H:300  45°W:180 H:280 |
| Saw blade speed(m/min) | 22/45/64 |
| Saw blade specific(mm) | 27x0.9x3505 |
| Voltage | 380V 50Hz 3P |
| Main motor(kw) | 2.2 |
| Hydraulic motor(kw) | 0.42 |
| Cooling motor(kw) | 0.04 |
| Saw blade tension way | Manual |
| Vice clamp way | Hydraulic with manual |
| Hydraulic oil tank | 40L |
| Machine weight(kg) | 800 |
| Voltage | 1830x1070x1400 |